; ######################################################################################
;
;  Fargo Printer Driver
;  Fargo DTC1250e Printer INF for Windows XP; Windows Server 2003; Windows Vista;  Windows 7; Server 2008R1; Windows Server 2008R2; Windows 8; Windows Server 2012
;  Copyright (c)  HID Global  2002-2014
;
; ######################################################################################

[Version]
Signature="$Windows NT$"
Provider=%OEM%

ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Class=Printer

CatalogFile=DTC1250e_x64.cat

DriverVer=02/28/2014, 2.2.0.4




[SourceDisksNames.amd64]
1   = %Disk1%,,,""



[SourceDisksFiles.amd64]
DTC1250eGR.dll   = 1
DTC1250eUI.dll   = 1
DTC1250eLM.dll   = 1
DTC1250eResEN.dll  = 1
DTC1250ePNP.dll  = 1
DTC1250eHlp.hlp  = 1
DTC1250e_BO_Tst.prn  	= 1
DTC1250e_K_CLR_Tst.prn  	= 1
DTC1250e_K_PRM_Tst.prn  	= 1
DTC1250e_K_STD_Tst.prn  	= 1
DTC1250e_KO_Tst.prn  	= 1
DTC1250e_NONE_Tst.prn 	= 1
DTC1250e_YMCKO_Half_Tst.prn = 1
DTC1250e_YMCKO_Tst.prn  	= 1
DTC1250e_YMCKOK_Tst.prn  = 1
DTC1250e_YMCKOK_Half_Tst.prn = 1
DTC1250e_YMCKOKO_Half_Tst.prn = 1
DTC1250eIPN.bmp    = 1
DTC1250eIPR.bmp    = 1
DTC1250eILN.bmp    = 1
DTC1250eILR.bmp    = 1
DTC1250eLPN.bmp    = 1
DTC1250eLPR.bmp    = 1
DTC1250eLLN.bmp    = 1
DTC1250eLLR.bmp    = 1
DTC1250eColor.bmp  = 1
DTC1250etbo.exe    = 1
DTC1250eMon.exe    = 1
DTC1250eCLR.icm    = 1
DTC1250eCLR_L.icm  = 1



[DestinationDirs]
DefaultDestDir        = 66000
DTC1250eLM_COPY        = 66002
DTC1250e_COLOR_PROFILES = 66003
;DTC1250eCOI_COPY       = 11



[Manufacturer]
%Manufacturer%=FARGO,ntamd64


[FARGO.ntamd64]

;
; Driver Name             DDInstall Section      DeviceID (referred to as Hw-id)
; -----------             -----------------      -------------------------------
;
"DTC1250e Card Printer"   = DTC1250e_PNPX,    USBPRINT\HID_GlobalDTC1250e70D2,HID_GlobalDTC1250e70D2

; Old one for DTC1000 with UPnP hardware id.
;USBPRINT\Fargo_DTC10004A24,UMB\VEN_2301&DEV_DTC10004A24,Fargo_DTC10004A24


; NOTE - MAKE SURE THAT THERE ARE NO SPACES BETWEEN THE HW-IDS, JUST COMMA SEPERATED FIELDS.


; DDInstall for regular Ethernet / Plug and Play Extensions installations
[DTC1250e_PNPX.ntamd64]
CopyFiles   = DTC1250eCOPY, DTC1250eLM_COPY, DTC1250e_COLOR_PROFILES
DataSection = DTC1250eDATA




[DTC1250eDATA]
DriverFile      = DTC1250eGR.dll
DataFile        = DTC1250eGR.dll
ConfigFile      = DTC1250eUI.dll
HelpFile        = DTC1250eHLP.HLP
LanguageMonitor = %OEM_MONITOR%

[DTC1250e_COLOR_PROFILES]
DTC1250eCLR.icm,,,0x00000020  ; Copy only if new binary
DTC1250eCLR_L.icm,,,0x00000020  ; Copy only if new binary


[DTC1250eLM_COPY]
DTC1250eLM.dll,,,0x00000020   ; Copy only if new binary

[DTC1250eCOPY]
DTC1250eGR.dll
DTC1250eUI.dll
DTC1250eHlp.hlp
DTC1250e_BO_Tst.prn
DTC1250e_K_CLR_Tst.prn
DTC1250e_K_PRM_Tst.prn
DTC1250e_K_STD_Tst.prn
DTC1250e_KO_Tst.prn
DTC1250e_NONE_Tst.prn
DTC1250e_YMCKO_Half_Tst.prn
DTC1250e_YMCKO_Tst.prn
DTC1250e_YMCKOK_Tst.prn
DTC1250e_YMCKOK_Half_Tst.prn
DTC1250e_YMCKOKO_Half_Tst.prn
DTC1250eIPN.bmp
DTC1250eIPR.bmp
DTC1250eILN.bmp
DTC1250eILR.bmp
DTC1250eLPN.bmp
DTC1250eLPR.bmp
DTC1250eLLN.bmp
DTC1250eLLR.bmp
DTC1250eColor.bmp
DTC1250etbo.exe
DTC1250eMon.exe
DTC1250ePNP.dll
DTC1250eResEN.dll



[Strings]			; Default strings if no language specified
OEM="Fargo"
Disk1="DTC1250e Driver Setup Disk 1"
OEM_MONITOR="DTC1250e Language Monitor,DTC1250eLM.DLL"
Manufacturer = "Fargo"

;DriverName = "Fargo DTC1250e Card Printer"


;[Strings.0007]			; generic German (German German is 0407)
;Disk1="DTC1250e Treiber Setup Disk 1"
;
;
;[Strings.0009]			; English (USA English is 0409)
;Disk1="DTC1250e Driver Setup Disk 1"
;
;
;[Strings.000c]			; generic French (France French is 040c)
;Disk1="DTC1250e Le disque d'installation du pilote 1"
;
;
;[Strings.000a]			; generic Spanish (Mexico Spanish is 080a, Spain Spanish is 0c0a)
;Disk1="DTC1250e Controlador de disco de instalación de una"






