| # Histogram Channel
| To select the histogram channel to be shown in the Histogram Graph area, select the corresponding item in the drop-down list:
| The available values are: RGB or Gray — this channel shows the luminosity of image data. Red — this channel shows the image data of the red channel. Green — this channel shows the image data of the green channel. Blue — this channel shows the image data of the blue channel.
| ** The driver for this device does not provide the function Histogram Channel.