Port Setting Installation
For a device connected to a network or locally, set the port to be used, then install the driver. As well as using existing ports, you can also add Standard TCP/IP ports or network printer ports.

IMPORTANT
Be sure to log on as a member of Administrators when you start the computer.

NOTE
If you are using a device connected to a network using TCP/IP protocol, you can automatically search for a port to install the driver. For instructions, see "Network Connection."

1.
Start the installer → follow the instructions on the screen.
For details, see steps 1 to 3 of "Network Connection."
2.
Select [Manually Set Port to Install] → click [Next].
3.
Select any required items → Click [Next].
[UFRII XPS Printer Driver]: Select the driver to be installed.
[Process to Install Printer Driver]: This is displayed if there are already drivers installed. Select a process to apply to existing drivers if necessary.
4.
Select the devices you want to install from [Printer List] → click [Add].
5.
Verify that the device you selected in step 4. has been added to [Printer List for Driver Installation] → click [Next].
To delete a device from the list, select the device → click [Remove].
6.
Select a port.
If more than one device is selected, this dialog box will reappear to enable selection of different ports for other devices.
If you want to add a Standard TCP/IP port
If you want to add a network printer port
If you want to use an existing port

NOTE
If you do not know how to set ports, select a temporary port ([LPT1] etc.) from [Port], then click [Next] and proceed to step 7.. You can set the correct port after the installation has finished (see "Changing a Standard TCP/IP Port").

If you want to add a Standard TCP/IP port
Click [Add Port].
Select [Standard TCP/IP Port] in the [Add Port] dialog box → click [OK].
Click [Next] in the [Add Standard TCP/IP Printer Port Wizard].
Enter the name of the device or its IP address in [Printer Name or IP Address] (or [Hostname or IP address]) → click [Next].
For the name of the device, use the name by which the device is known on the network.
[Port Name] is automatically entered. Change the port name if required.
If the [Additional Port Information Required] (or [Additional port information required]) dialog box is displayed, follow one of the procedures below.
Return to the previous screen in the wizard → re-enter the information for [Printer Name or IP Address] (or [Hostname or IP address]) → click [Next].
Select [Standard] for [Device Type] → [Canon Network Printing Device with P9100] from the drop-down list → click [Next].
Click [Finish] → proceed to step 7..

NOTE
If you do not know the device name or IP address, contact your network administrator. The type of device you select from the [Standard] drop-down list under [Device Type] in the [Additional Port Information Required] (or [Additional port information required]) dialog box depends on the printer model you are using, and may differ from the above setting.

If you want to add a network printer port
Click [Add Port].
Select [Network] in the [Add Port] dialog box → click [OK].
Select the network printer to use → click [OK] → proceed to step 7..
If you want to use an existing port
Select a port from [Port] → proceed to step 7..
7.
Change [Printer Name] if required → select [Set as Default] to set the device as the default device → click [Next].
If you want to specify shared printer settings, select [Use as Shared Printer] (see "Print Server Settings").
If you have added a network printer port in step 6., you cannot set [Printer Name] and [Use as Shared Printer].
8.
Verify [Printer List for Driver Installation] → click [Start].
9.
Click [Exit] (or [Restart]).
The installed device(s) are displayed in [Devices and Printers] (or [Printers and Faxes] or [Printers]) in the Windows Control Panel.
The driver is now installed.