;
; MX880F6.INF (for Windows x64 Monolithic driver)
;
; List of supported facsimiles, manufacturers
;

[Version]
Signature="$Windows NT$"
Provider=%CANON%
ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Class=Printer
CatalogFile=MX880F6.CAT
DriverVer=03/27/2012, 10.00.2.20

;
; Manufacturer section.
;
; This section lists all of the manufacturers
; that we will display in the Dialog box
;

[Manufacturer]
%CANON%=Models,NTamd64.5.1,NTamd64.6.0

;
; Model sections.
;
; Each section here corresponds with an entry listed in the
; [Manufacturer] section, above. The models will be displayed in the order
; that they appear in the INF file.
;


; x86AdditionalDriver
[Models]
%CN_DRIVERNAME%=FAX_INSTALL,USBPRINT\CanonMX880_series_FA4893

; WindowsXP
[Models.NTamd64.5.1]
%CN_DRIVERNAME%=FAX_INSTALL,USBPRINT\CanonMX880_series_FA4893

; WindowsVista
; Windows7
[Models.NTamd64.6.0]
%CN_DRIVERNAME%=FAX_INSTALL,USBPRINT\CanonMX880_series_FA4893
%CN_DRIVERNAME%=FAX_INSTALL,WSDPRINT\CanonMX880_series_FA4893

[FAX_INSTALL]
DataSection = COMMON_DATA
CopyFiles   = FAX_DRV, FAX_LM, FAX_ADDBK, OPTLANGUAGE

[COMMON_DATA]
DriverFile      = CNCADAN.DLL
ConfigFile      = CNCAUAN.DLL
DataFile        = CNCAIAN.INI
;HelpFile        = CNCAHAN.CHM
LanguageMonitor = %CN_LANGUAGEMONITOR%

; Copy Sections
;
; Lists of files that are actually copied. These sections are referenced
; from the installer sections, above. Only create a section if it contains
; two or more files (if we only copy a single file, identify it in the
; installer section, using the @filename notation) or if it's a color
; profile (since the DestinationDirs can only handle sections, and not
; individual files).
;

[FAX_DRV]
CNCADAN.DLL,FXDR.DLL
CNCAUAN.DLL,FXUI.DLL
CNCARAN.DLL,FXUR.DLL
CNCAIAN.INI,MX880.INI

[FAX_ADDBK]
CNCA0AN.DLL,FXAD.DLL
CNCA1AN.DLL,FXAR.DLL
CNCA2AN.DLL,FXWA.DLL

[FAX_LM]
CNCALAN.DLL,FXLM.DLL,,0x00000020    ; Copy only if new binary

[OPTLANGUAGE]
CNCARAN0.411,FXURJ.DLL
CNCARAN0.40c,FXURFR.DLL
CNCARAN0.407,FXURDE.DLL
CNCARAN0.410,FXURIT.DLL
CNCARAN0.c0a,FXURES.DLL
CNCARAN0.816,FXURPT.DLL
CNCARAN0.406,FXURDK.DLL
CNCARAN0.414,FXURNO.DLL
CNCARAN0.41D,FXURSE.DLL
CNCARAN0.40b,FXURFI.DLL
CNCARAN0.408,FXURGR.DLL
CNCARAN0.415,FXURPL.DLL
CNCARAN0.405,FXURCZ.DLL
CNCARAN0.419,FXURRU.DLL
CNCARAN0.40e,FXURHU.DLL
CNCARAN0.413,FXURNL.DLL
CNCARAN0.41F,FXURTR.DLL
CNCARAN0.401,FXURAR.DLL
CNCARAN0.804,FXURCN.DLL
CNCARAN0.404,FXURTW.DLL
CNCARAN0.412,FXURKR.DLL
CNCARAN0.41E,FXURTH.DLL
CNCARAN0.421,FXURID.DLL

;
; Call SetupSetDirectoryId with 66000 to set the target directory at runtime
; (depending on which environment drivers are getting installed)
;

[DestinationDirs]
DefaultDestDir=66000
FAX_LM=66002

;
;  Source Disk Section
;  This was added to enable Web Point&Print.
;  All files added to this must also be added to Layout.INF
;
[SourceDisksNames.amd64]
1=%DISK1%,"FAXG6.CAB",,,0x10,"MX880F6.CAT"

[SourceDisksFiles]
FXDR.DLL      = 1
FXUI.DLL      = 1
FXLM.DLL      = 1
FXUR.DLL      = 1
FXURJ.DLL     = 1
FXURES.DLL    = 1
MX880.ini     = 1
FXAD.DLL      = 1
FXAR.DLL      = 1
FXWA.DLL      = 1
FXURFR.DLL    = 1
FXURDE.DLL    = 1
FXURIT.DLL    = 1
FXURPT.DLL    = 1
FXURDK.DLL    = 1
FXURNO.DLL    = 1
FXURSE.DLL    = 1
FXURFI.DLL    = 1
FXURGR.DLL    = 1
FXURPL.DLL    = 1
FXURCZ.DLL    = 1
FXURRU.DLL    = 1
FXURHU.DLL    = 1
FXURNL.DLL    = 1
FXURTR.DLL    = 1
FXURAR.DLL    = 1
FXURCN.DLL    = 1
FXURTW.DLL    = 1
FXURKR.DLL    = 1
FXURTH.DLL    = 1
FXURID.DLL    = 1

; Localizable Strings
;
[Strings]
CANON="Canon"
CN_LANGUAGEMONITOR="Canon BJ FAX Language Monitor MX880 series,CNCALAN.DLL"
CN_DRIVERNAME="Canon MX880 series FAX"
DISK1="Canon MX880 series Setup Disk"
