| iPF815/iPF825 Paper Reference Guide (for EU) |  |

| This paper reference guide describes the types of paper printable with Canon imagePROGRAF iPF815/iPF825. Before using the printer and paper, read through this guide, the instruction manual supplied with the paper and the printer's User Manual for use in optimal conditions.

> Local Availability of Paper in This Guide
This guide includes information for paper sold in EU. Some paper in the guide may not be available locally, depending on your location.
> Printer Operations
For instructions on loading or cutting paper or other printer operations, refer to the User Manual.
> Updating the Paper Reference Guide
The Paper Reference Guide is automatically updated when you update the Media Configuration Tool. To download the latest version of the Media Configuration Tool, access the imagePROGRAF website from imagePROGRAF Support Information. If information for paper you have added using the Media Configuration Tool is not included in this guide, refer to the guide specifically for that paper. (→View information for media types you have added)
> Genuine Canon Paper
The paper types with "†" marked in the product name are those specified as genuine Canon paper. For other paper, please contact the respective paper manufacturer after reading the instruction manuals supplied with the paper.
> Handling the Paper
Handle all paper carefully and avoid moist environment and contact with water. If the paper will be used in a humid environment, perform lamination or other appropriate treatments after printing. Handle all paper carefully, being careful not to rub or damage it. We recommend wearing gloves when handling paper. Handle paper so as to keep the print surface free of sweat and grease from hands. This may affect the printing quality. After printing, allow ink to dry before handling. We recommend keeping printed documents separate, not stacked, until they are dry. Paper may stretch or shrink from changes in humidity or other environmental factors. Allow ample time for the paper to adjust to the environment before use. After use, remove paper from the printer if environmental changes are expected and store it in the bag.
> Loading Rolls
Unaligned roll edges, stains and tape marks may lead to faulty paper feeding. If the roll edge is curled, straighten the curled edge before loading the roll.
> Precaution when using rolls with significant curling
The printed surface of rolls with significant curling of the leading edge may become soiled. Straighten out these rolls before use. If the curling cannot be removed, advance the paper using the printer's control panel until the edge of the roll emerges from the top cover before printing. For printer operating instructions, see the printer's User Manual.
> Ejecting Roll Paper
Depending on the condition of paper after ejection, ejected sheets may impede ejection of the next sheet or damage other sheets. Remove each sheet after ejection.
> If Paper Cannot be Selected
If the type of paper loaded cannot be selected on the control panel or in the printer driver, try specifying it as Special 1, Special 2, and so on. Note that higher numbers in this setting enable more vivid colors but may also cause colors to run together.
> Cutting Options for Rolls That Take Time for Ink to Dry (Eject Cut)
Ink takes longer to dry on paper for which Auto Cutting is labeled "Eject cut" in the Roll Specification section. If you use automatic cutting after printing and the document drops, ink may rub off the printed surface. Support the document after printing as you wait for the printer to cut it. For detailed instructions, refer to the printer's User Manual.
> HP-GL/2
Paper types marked with "Yes" in the HP-GL/2 column support HP-GL/2 output. For detailed instructions, refer to the printer's User Manual.
> Operating Environment
If used in other than the recommended environment, your printer may develop the following problems: Be sure to conduct printing in the recommended operating environment. <Low Humidity Environment> Paper becomes curled or wrinkled. Paper and the printhead are more likely to touch each other, resulting in a scratched print surface or damaged printhead. The cut printed matter sticks to the printer and will not fall down (film media). Paper sticks to the printer, making its transfer impossible and preventing its normal ejection (film media). Uneven printing (film media) <High Humidity Environment> Printed matter will not dry. Wavy paper surface Cut edges are ragged (fabric media). Margins remain due to borderless printing. Print under a humidity of 60% or lower.
Plain Paper
Suitable for color prints for project presentations or monochrome prints for ceremony programs in schools. Thanks to its low cost, it is also applicable to test printing. Product Specifications
Category | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
Plain Paper | Roll | Plain Paper (*1) | Plain Paper (*2) | MBK | Temperature 15-30°C Humidity 10-80%
Plain Paper (High Grade) | Roll | Plain Paper HG (*1) | Plain Paper (High Grade) (*2) | MBK | Temperature 15-30°C Humidity 10-80%
Premium Plain Paper 80 | Roll | PremPlainPpr 80 | Premium Plain Paper 80 | MBK | Temperature 15-30°C Humidity 10-60%
Premium Plain Paper 80 (for Borderless Printing) | Roll | Prem80forBrdrlss | PremPlainPpr 80(forBrdrlss Prt.) | BK | Temperature 15-30°C Humidity 10-60%
Precautions Premium Plain Paper 80 If the color is uneven, it is recommended to select Unidirectional Printing in Advanced Settings of the printer driver, or set Print Quality to High before performing printing.
Somewhat less black ink will be used if you choose PlainP_ConsMBK (*1) or All Plain Paper_Conserve MBK (*2). Try this setting if ink smearing is a concern. This setting is available for Plain Paper and Plain Paper (High Grade).
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
Plain Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
Plain Paper (High Grade) | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A2 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A1 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A0 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
Premium Plain Paper 80 | 17 in. | Yes (*2) | Yes | No | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes (*3)
24 in. | Yes (*2) | Yes | No | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes (*3)
36 in. | Yes (*2) | Yes | No | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes (*3)
42 in. | Yes (*2) | Yes | No | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes (*3)
A2 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes (*3)
A1 | Yes (*2) | Yes | No | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes (*3)
A0 | Yes (*2) | Yes | No | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes (*3)
B2 | Yes (*2) | Yes | No | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes (*3)
B1 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes (*3)
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper. *2: This is possible when the printer driver is set to PremPlainPpr 80(forBrdrlss Prt.) and the control panel is set to Prem80forBrdrlss. Select the Borderless Printing check box in the printer driver page setup sheet. *3: When printing in HP-GL2 mode, set the printer driver to Premium Plain Paper 80 and set the control panel to PremPlainPpr 80.
Recycled Paper
Paper with a 70% blending ratio of used paper pulp. This versatile paper supports various applications including CAD, presentation graphics, easy posters, point-of-purchase displays, and advertising flyers or leaflets. Product Specifications
Category | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
Plain Paper | Roll | Plain Paper | Plain Paper | MBK | Temperature 15-30°C Humidity 10-80%
Recycled Coated Paper | Roll | Recycled Coated | Recycled Coated Paper | BK | Temperature 15-30°C Humidity 10-80%
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
Plain Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A2 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A1 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A0 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
Recycled Coated Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper.
Coated Paper
Paper-based coated paper. Coated paper is a good choice for line drawings, maps, perspective drawings, and presentation graphics. Heavyweight Coated Paper provides sharp graphic and full-color images. It has a wide range of uses, including point-of-purchase displays. Extra Heavyweight Coated Paper is heavier than ordinary heavyweight coated paper, with a distinctive texture. Premium Matte Paper is high-resolution extra heavyweight matte coated paper offering a wide color reproducibility. Reflection-free and giving a placid look and feel, its uses range from photos and fine art to high-resolution posters and point-of-purchase displays. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
Coated Paper | - | Roll | Coated Paper | Coated Paper | BK | Temperature 15-30°C Humidity 10-80%
Heavyweight Coated Paper | - | Roll | HW Coated | Heavyweight Coated Paper | BK | Temperature 15-30°C Humidity 10-80%
Extra Heavyweight Coated Paper | - | Roll | Ex HW Coated | Extra Heavyweight Coated Paper | BK | Temperature 15-30°C Humidity 10-80%
Premium Matte Paper | - | Roll | Premium MatteP | Premium Matte Paper | BK | Temperature 15-30°C Humidity 30-80%
Colored Coated Paper | - | Roll | Colored Coated | Colored Coated Paper | MBK | Temperature 15-30°C Humidity 10-80%
Matte Coated Paper 90gsm | Matt Coated Paper 90gsm (†) | Roll | Matte Coated 90 | Matte Coated Paper 90gsm | BK | Temperature 15-30°C Humidity 10-80%
Matt Coated Paper | Matt Coated Paper 9171 (†) | Roll | Matt Coated P | Matt Coated Paper | BK | Temperature 15-30°C Humidity 10-80%
Matt Coated Paper 140g | Matt Coated Paper 140g (†) | Roll | Matt Coat 140g | Matt Coated Paper 140g | BK | Temperature 15-30°C Humidity 30-80%
Extra Matt Coated Paper | Matt Coated Paper 7215 (†) | Roll | Extra Matt Coat | Extra Matt Coated Paper | BK | Temperature 15-30°C Humidity 10-80%
Opaque Paper | Opaque paper White (†) | Roll | Opaque Paper | Opaque Paper | BK | Temperature 15-30°C Humidity 10-80%
Hi Res Graphic Paper | High Resolution Graphic paper Self ADH (†) | Roll | Hi Res Gra P | Hi Res Graphic Paper | BK | Temperature 15-30°C Humidity 10-80%
Hi Res Barrier Paper | High Resolution Barrier Paper (†) | Roll | Hi Res BarrierP | Hi Res Barrier Paper | BK | Temperature 15-30°C Humidity 30-80%
Precautions Coated Paper Depending on the condition of paper after ejection, ejected sheets may impede ejection of the next sheet. Remove each sheet after ejection.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
Coated Paper | 24 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Heavyweight Coated Paper | 24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
A2 | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
A1 | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
A0 | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
B2 | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
B1 | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Extra Heavyweight Coated Paper | 24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
Premium Matte Paper | 17 in. | Yes | Yes | Yes | Off | Not required | 150 mm | 150 mm | 150 mm | 150 mm | Yes
24 in. | Yes | Yes | Yes | Off | Not required | 150 mm | 150 mm | 150 mm | 150 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 150 mm | 150 mm | 150 mm | 150 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 150 mm | 150 mm | 150 mm | 150 mm | Yes
Colored Coated Paper | 24 in. | No | Yes | Yes | Off | Not required | 100 mm | 250 mm | - | - | No
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 250 mm | - | - | No
Matte Coated Paper 90gsm | 24 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
42 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Matt Coated Paper | 24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
Matt Coated Paper 140g | 17 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
Extra Matt Coated Paper | 17 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
Opaque Paper | 17 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
Hi Res Graphic Paper | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Hi Res Barrier Paper | 17 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | Yes
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper.
Photo Paper
Having a gloss like photographic paper for silver halide photos, Glossy Photo Paper is suitable for high-definition photo images. This paper is resin-coated, preventing problems from ink absorption and ensuring a flat finish. Semi-Glossy Photo Paper is glossy white paper less reflective than regular glossy photo paper. The soft finish of this paper is subdued, for minimal glare. Its low reflectivity makes it a good choice for display panels and presentation graphics at exhibitions, or for point-of-purchase displays. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
Glossy Photo Paper HG 170 | Glossy Photo Paper HG 170 (†) | Roll | GlossyPhotoHG170 | Glossy Photo Paper HG 170 | BK | Temperature 15-30°C Humidity 30-80%
Semi-Glossy Photo Paper HG 170 | Semi-Glossy Photo Paper HG 170 (†) | Roll | SemGlsPhotoHG170 | Semi-Glossy Photo Paper HG 170 | BK | Temperature 15-30°C Humidity 30-80%
Glossy Photo Paper HG 255 | Glossy Photo Paper HG 255 (†) | Roll | GlossyPhotoHG255 | Glossy Photo Paper HG 255 | BK | Temperature 15-30°C Humidity 30-80%
Semi-Glossy Photo Paper HG 255 | Semi-Glossy Photo Paper HG 255 (†) | Roll | SemGlsPhotoHG255 | Semi-Glossy Photo Paper HG 255 | BK | Temperature 15-30°C Humidity 30-80%
Premium Glossy Paper 280 | Premium Glossy Paper 280 (†) | Roll | Premium Gl 280 | Premium Glossy Paper 280 | BK | Temperature 15-30°C Humidity 30-80%
Premium Semi-Glossy Paper 280 | Premium Semi-Glossy Paper 280 (†) | Roll | Prem.SemiGl 280 | Premium Semi-Glossy Paper 280 | BK | Temperature 15-30°C Humidity 30-80%
Glossy Photographic Paper 190gsm | Photo Quality Paper Glossy 190gsm (†) | Roll | GlossyPhoto 190 | Glossy Photographic Paper 190gsm | BK | Temperature 15-30°C Humidity 30-60%
Glossy Photographic Paper 240gsm | Photo Quality Paper Glossy 240gsm (†) | Roll | GlossyPhoto 240 | Glossy Photographic Paper 240gsm | BK | Temperature 15-30°C Humidity 30-60%
Glossy Photographic Paper 270gsm | Photo Quality Paper Glossy 270gsm (†) | Roll | GlossyPhoto 270 | Glossy Photographic Paper 270gsm | BK | Temperature 15-30°C Humidity 30-80%
HW Glossy Photo Paper | Photo Quality Paper Glossy 300gsm (†) | Roll | HW Gloss Photo | HW Glossy Photo Paper | BK | Temperature 15-30°C Humidity 30-60%
Satin Photographic Paper 190gsm | Photo Quality Paper Satin 190gsm (†) | Roll | SatinPhoto 190 | Satin Photographic Paper 190gsm | BK | Temperature 15-30°C Humidity 30-60%
Satin Photographic Paper 240gsm | Photo Quality Paper Satin 240gsm (†) | Roll | SatinPhoto 240 | Satin Photographic Paper 240gsm | BK | Temperature 15-30°C Humidity 30-60%
Photo paper Pearl 260g | Photo paper Pearl 260g (†) | Roll | Photo Pearl | Photo paper Pearl 260g | BK | Temperature 15-30°C Humidity 30-80%
Satin Photographic Paper 270gsm | Photo Quality Paper Satin 270gsm (†) | Roll | SatinPhoto 270 | Satin Photographic Paper 270gsm | BK | Temperature 15-30°C Humidity 30-80%
HW Satin Photo Paper | Photo Quality Paper Glacier 300gsm (†) | Roll | HW Satin Photo | HW Satin Photo Paper | BK | Temperature 15-30°C Humidity 30-60%
Precautions Photo Quality Paper Satin 190gsm The first document printed after loading a roll may be wrinkled.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
Glossy Photo Paper HG 170 | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
A1 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
A0 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
B2 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
B1 | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
Semi-Glossy Photo Paper HG 170 | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
A1 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
A0 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
B2 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
B1 | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
Glossy Photo Paper HG 255 | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Semi-Glossy Photo Paper HG 255 | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Premium Glossy Paper 280 | 10 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Premium Semi-Glossy Paper 280 | 10 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Glossy Photographic Paper 190gsm | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Glossy Photographic Paper 240gsm | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Glossy Photographic Paper 270gsm | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
HW Glossy Photo Paper | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Satin Photographic Paper 190gsm | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Satin Photographic Paper 240gsm | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Photo paper Pearl 260g | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Satin Photographic Paper 270gsm | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
HW Satin Photo Paper | 17 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper.
Synthetic Paper
Highly economical synthetic paper using polypropylene-based film, a material suited for display posters. Can be displayed outdoors if laminated. Product Specifications
Category | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
Synthetic Paper | Roll | Syn. Paper | Synthetic Paper | BK | Temperature 15-30°C Humidity 30-80%
Adhesive Synthetic Paper | Roll | Adh. Syn. Paper | Adhesive Synthetic Paper | BK | Temperature 15-30°C Humidity 10-80%
Precautions Adhesive Synthetic Paper If the leading edge of Adhesive Synthetic Paper curls upward, the adhesive may stick to the printhead and damage it. In this case, take measures to straighten the paper, such as by cutting the leading edge.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
Synthetic Paper | 24 in. | No | Yes | Yes (*2) | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes (*2) | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes (*2) | Off | Required | 100 mm | 100 mm | - | - | No
Adhesive Synthetic Paper | 24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper. *2: Media Take-up unit can be used up to max. 60% humidity.
Film
Print on the glossy, translucent front. With light shined from the back, it s used for indoor illumination signboards and vivid displays. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
Backlit Film | Back Light Film (†) | Roll | Backlit Film | Backlit Film | BK | Temperature 15-30°C Humidity 10-80%
Precautions Avoid using Backlit Film where the print surface becomes wet. If the media will be used in a humid environment, perform lamination or other appropriate treatments after printing. When printing on Backlit Film, set Print Quality to Standard or High in the printer driver. Printing may appear uneven, but this effect will be softened by backlighting.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
Backlit Film | 24 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
36 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
42 in. | No | Eject cut | Yes | Off | Required | - | - | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper.
Proofing
Proofing paper supports the color reproduction gamut for proof offset printing, providing color comparable to a print finish. It is best suited for color proofing print for printing tasks. Newsprint for proofing offers a look and feel close to newsprint and supports a wide color reproduction gamut. Thanks to its low cost, it is also applicable to test printing. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
Proofing Paper | - | Roll | Proofing Paper | Proofing Paper | BK | Temperature 15-30°C Humidity 30-80%
Newsprint for Proofing 1 | - | Roll | News Proof 1 | (*1) | MBK | Temperature 15-30°C Humidity 10-80%
Newsprint for Proofing 2 | - | Roll | News Proof 2 | (*1) | MBK | Temperature 15-30°C Humidity 10-80%
Glossy Proofing Paper 195g | Professional Proof and Photo Glossy 195g (†) | Roll | Glossy Proofing | Glossy Proofing Paper 195g | BK | Temperature 15-30°C Humidity 10-60%
Semiglossy Proofing Paper 195g | Professional Proof and Photo Semiglossy 195g (†) | Roll | SemiGlProof 195 | Semiglossy Proofing Paper 195g | BK | Temperature 15-30°C Humidity 10-60%
Commercial Proofing Paper | Proofing Paper Glossy 200gsm (†) | Roll | Comm Proofing | Commercial Proofing Paper | BK | Temperature 15-30°C Humidity 30-80%
Semiglossy Proofing Paper 255g | Professional Proof and Photo Semiglossy 255g (†) | Roll | SemiGlProof 255 | Semiglossy Proofing Paper 255g | BK | Temperature 15-30°C Humidity 30-80%
Precautions If print quality is your priority, turn off the auto cutting function and stop the printer after printing. We recommend supporting the document with your hands to prevent it from dropping before you press the Stop button and cut the paper.
*1: The optional RIP software is required.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
Proofing Paper | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Newsprint for Proofing 1 | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
Newsprint for Proofing 2 | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
Glossy Proofing Paper 195g | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
Semiglossy Proofing Paper 195g | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
Commercial Proofing Paper | 24 in. | No | Yes | Yes | Off | Required | 100 mm | 320 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 320 mm | - | - | No
42 in. | No | Yes | Yes | Off | Required | 100 mm | 320 mm | - | - | No
Semiglossy Proofing Paper 255g | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper.
CAD Paper
This paper is a good choice for CAD graphic (line drawing) prints. CAD Tracing Paper is thin, translucent paper that can be used in color printing. CAD Translucent Matte Film offers high dimensional stability, making it suited for high-precision prints such as master drawings. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment
CAD Tracing Paper | - | Roll | CAD Trace Paper | CAD Tracing Paper | MBK | Temperature 15-30°C Humidity 30-80%
CAD Translucent Matte Film | - | Roll | CAD Matte Film | CAD Translucent Matte Film | MBK | Temperature 15-30°C Humidity 10-80%
CAD Clear Film | - | Roll | CAD Clear Film | CAD Clear Film | BK | Temperature 15-30°C Humidity 30-60%
Standard Paper1569B 80g | Standard Paper1569B 80g (†) | Roll | Standard P 80g | Standard Paper1569B 80g | MBK | Temperature 15-30°C Humidity 30-80%
Standard Paper1570B 90g | Standard Paper1570B 90g (†) | Roll | Standard P 90g | Standard Paper1570B 90g | MBK | Temperature 15-30°C Humidity 10-80%
Precautions CAD Tracing Paper Remove each sheet upon ejection into the output tray. Do not touch the print surface or stack sheets before ink dries. If the ink does not dry easily, set Roll DryingTime to about a minute. CAD Clear Film If you are using automatic detection of the remaining roll paper with CAD Clear Film, before printing, manually cut the portion of the film that includes the media name or other text.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | HP-GL/2
When loading paper (*1) | Borderless printing
Low/Normal humidity | High humidity | Low/Normal humidity | High humidity
CAD Tracing Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A2 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A1 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
A0 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
CAD Translucent Matte Film | 36 in. | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | Yes
A1 | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | Yes
A0 | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | Yes
CAD Clear Film | 36 in. | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | Yes
Standard Paper1569B 80g | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
Standard Paper1570B 90g | 17 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | Yes
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Off is the default setting for most types of paper.
Type: | Shows the paper type. The properties are given in a separate table according to the type.
Control Panel: | On the iPF815, the types of paper that can be selected in Roll Media Type and Cut Sheet Type on the control panel are indicated. On the iPF825, the types of paper that can be selected in Roll1(Uppr) Type, Roll2 (Lwr) Type, and Cut Sheet Type on the control panel are indicated.
Printer Driver: | Shows the paper types selected in Media Type of the printer driver.
Black Ink: | Shows the black ink types used.
Recommended Environment: | Shows the temperature and humidity ranges for using paper.
Borderless Printing: | Shows whether borderless printing is possible.
Auto Cutting: | Shows the method of paper cutting.
Media Take-up Unit: | Indicates that the media take-up unit cannot be used.
Ink Drying Time: | Shows the ink drying time when using the cutter. Set the printer's ink drying time according to this table.
Edge Precut Paper Removal: | Required is indicated for paper for which you must remove scraps produced when the leading edge is cut. Remove these scraps from the platen or output stacker before printing.
Edge Precut Length: | Indicates the edge precut length for roll paper.
HP-GL/2: | Shows whether HP-GL/2 output is supported.
Precautions: | Shows the precautions and limitations for each paper type.
The information given here is current as of end of June, 2010 and subject to change at any time.
To purchase paper, contact your printer distributor.
Copyright Canon Inc. 2010