| iPF9010S/iPF9110 Paper Reference Guide (for North or South America) |  |

| This paper reference guide describes the types of paper printable with Canon imagePROGRAF iPF9010S/iPF9110. Before using the printer and paper, read through this guide, the instruction manual supplied with the paper and the printer's User Manual for use in optimal conditions.

> Local Availability of Paper in This Guide
This guide includes information for paper sold in North or South America. Some paper in the guide may not be available locally, depending on your location.
> Printer Operations
For instructions on loading or cutting paper or other printer operations, refer to the User Manual.
> Updating the Paper Reference Guide
The Paper Reference Guide is automatically updated when you update the Media Configuration Tool. To download the latest version of the Media Configuration Tool, access the imagePROGRAF website from imagePROGRAF Support Information.
> Genuine Canon Paper
The paper types with "†" marked in the product name are those specified as genuine Canon paper. For other paper, please contact the respective paper manufacturer after reading the instruction manuals supplied with the paper.
> Handling the Paper
Handle all paper carefully, being careful not to rub or damage it. We recommend wearing gloves when handling paper. Handle paper so as to keep the print surface free of sweat and grease from hands. This may affect the printing quality. After printing, allow ink to dry before handling. We recommend keeping printed documents separate, not stacked, until they are dry. After printing, handle prints carefully and avoid touching the print surface. Due to their nature, pigment inks may flake off if rubbed or scratched. Paper may stretch or shrink from changes in humidity or other environmental factors. Allow ample time for the paper to adjust to the environment before use. After use, remove paper from the printer if environmental changes are expected and store it in the bag.
> Loading Rolls
Unaligned roll edges, stains and tape marks may lead to faulty paper feeding. If the roll edge is curled, straighten the curled edge before loading the roll.
> Ejecting Roll Paper
Depending on the condition of paper after ejection, ejected sheets may impede ejection of the next sheet or damage other sheets. Remove each sheet after ejection.
> If Paper Cannot be Selected
If the type of paper loaded cannot be selected on the control panel or in the printer driver, try specifying paper for which "BK" is indicated in the Black Ink column as a special paper (Special Paper 1 to 5), or try specifying paper for which "MBK" is indicated as Special 6 to Special 10.
> Cutting Options for Rolls That Take Time for Ink to Dry (Eject Cut)
Ink takes longer to dry on paper for which Auto Cutting is labeled "Eject cut" in the Roll Specification section. If you use automatic cutting after printing and the document drops, ink may rub off the printed surface. Support the document after printing as you wait for the printer to cut it. For detailed instructions, refer to the printer's User Manual.
> Color Calibration
Color calibration is a feature that compensates for changes in color from individual variation among Printheads or from the printing environment, ensuring better color consistency. Although paper labeled with "No" in the Color Calibration column cannot be used to perform color calibration (that is, to print the patterns for adjustment), the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper. For detailed instructions, refer to the printer's User Manual.
> Operating Environment
If used in other than the recommended environment, your printer may develop the following problems: Be sure to conduct printing in the recommended operating environment. <Low Humidity Environment (below 30%)> Paper becomes curled or wrinkled. Paper and the printhead are more likely to touch each other, resulting in a scratched print surface or damaged printhead. The cut printed matter sticks to the printer and will not fall down (film media). Paper sticks to the printer, making its transfer impossible and preventing its normal ejection (film media). Uneven printing (film media) <High Humidity Environment (over 60%)> Printed matter will not dry. Wavy paper surface Cut edges are ragged (fabric media). Margins remain due to borderless printing.
Plain Paper
Suitable for color prints for project presentations or monochrome prints for ceremony programs in schools. Thanks to its low cost, it is also applicable to test printing. Plain Paper (High Quality) is exceptionally white, heavyweight paper designed for ink-jet printing. Product Specifications
Category | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Plain Paper | Roll | Plain Paper | Plain Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Plain Paper (High Quality) | Roll | Plain Paper HQ | Plain Paper (High Quality) | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Plain Paper (High Grade) | Roll | Plain Paper HG | Plain Paper (High Grade) | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Precautions Avoid using Plain Paper and Plain Paper (High Quality) in environments where the paper may get wet.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Plain Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
Plain Paper (High Quality) | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
Plain Paper (High Grade) | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A2 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A1 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A0 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper.
Recycled Paper
Paper with a 70% blending ratio of used paper pulp. This versatile paper supports various applications including CAD, presentation graphics, easy posters, point-of-purchase displays, and advertising flyers or leaflets. Product Specifications
Category | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Plain Paper | Roll | Plain Paper | Plain Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Recycled Coated Paper | Roll | Recycled Coated | Recycled Coated Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Precautions Avoid using Plain Paper in environments where the paper may get wet.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Plain Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A2 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A1 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A0 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
Recycled Coated Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper.
Coated Paper
Paper-based coated paper. Coated paper is a good choice for line drawings, maps, perspective drawings, and presentation graphics. Heavyweight Coated Paper provides sharp graphic and full-color images. It has a wide range of uses, including point-of-purchase displays. Extra Heavyweight Coated Paper is heavier than ordinary heavyweight coated paper, with a distinctive texture. Premium Matte Paper is high-resolution extra heavyweight matte coated paper offering a wide color reproducibility. Reflection-free and giving a placid look and feel, its uses range from photos and fine art to high-resolution posters and point-of-purchase displays. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Coated Paper | - | Roll | Coated Paper | Coated Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Heavyweight Coated Paper | Heavyweight Coated Paper (†) | Roll | HW Coated | Heavyweight Coated Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Extra Heavyweight Coated Paper | - | Roll | Ex HW Coated | Extra Heavyweight Coated Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Premium Matte Paper | Premium Matte Paper (†) | Roll | Premium MatteP | Premium Matte Paper | MBK | Temperature 59-86°F Humidity 40-80% | Applicable
Colored Coated Paper | - | Roll | Colored Coated | Colored Coated Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Matte Coated Paper 90gsm | Matte Coated Paper 90gsm | Roll | Matte Coated 90 | Matte Coated Paper 90gsm | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Premium Coated Paper | High Resolution Coated Paper | Roll | Premium Coated | Premium Coated Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Matte Coated Paper 170gsm | Matte Coated Paper 170gsm | Roll | MatteCoated 170 | Matte Coated Paper 170gsm | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Precautions If print quality is your priority, turn off the auto cutting function and stop the printer after printing. We recommend supporting the document with your hands to prevent it from dropping before you press the Stop button and cut the paper. Coated Paper Depending on the condition of paper after ejection, ejected sheets may impede ejection of the next sheet. Remove each sheet after ejection.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Coated Paper | 24 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Heavyweight Coated Paper | 24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
50 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
A2 | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
A1 | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
A0 | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
B2 | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
B1 | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Extra Heavyweight Coated Paper | 24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | No
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | No
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | No
Premium Matte Paper (*3) | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
60 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Colored Coated Paper | 24 in. | No | Yes | Yes | Off | Not required | 100 mm | 250 mm | - | - | No
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 250 mm | - | - | No
Matte Coated Paper 90gsm | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Premium Coated Paper | 24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
Matte Coated Paper 170gsm | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 320 mm | - | - | No
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | No
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | No
42 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 320 mm | 100 mm | 320 mm | No
60 in. | No | Yes | Yes | Off | Not required | 100 mm | 320 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper. *3: By default, NearEnd RollMrgn on the printer is set to 20mm, but you can also change it to 5mm. If you specify 5mm, for best results, use the printer under the recommended environmental conditions.
Photo Paper
Having a gloss like photographic paper for silver halide photos, Glossy Photo Paper is suitable for high-definition photo images. This paper is resin-coated, preventing problems from ink absorption and ensuring a flat finish. Semi-Glossy Photo Paper is glossy white paper less reflective than regular glossy photo paper. The soft finish of this paper is subdued, for minimal glare. Its low reflectivity makes it a good choice for display panels and presentation graphics at exhibitions, or for point-of-purchase displays. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Glossy Photo Paper (*1) | - | Roll | Glossy Photo | Glossy Photo Paper | BK | Temperature 59-86°F Humidity 30-80% | Applicable
Semi-Glossy Photo Paper (*1) | - | Roll | Semi-Gl Photo | Semi-Glossy Photo Paper | BK | Temperature 59-86°F Humidity 30-80% | Applicable
Premium Glossy Paper 200 (*1) | Premium Glossy Paper 200 (†) | Roll | Premium Gl 200 | Premium Glossy Paper 200 | BK | Temperature 59-86°F Humidity 30-80% | Applicable
Premium Semi-Glossy Paper 200 (*1) | Premium Semi-Glossy Paper 200 (†) | Roll | Prem.SemiGl 200 | Premium Semi-Glossy Paper 200 | BK | Temperature 59-86°F Humidity 30-80% | Applicable
Heavyweight Glossy Photo Paper 2 | - | Roll | HW GlossyPhoto2 | Heavyweight Glossy Photo Paper 2 | BK | Temperature 59-86°F Humidity 10-80% | Applicable
Heavywght SemiGlos Photo Paper 2 | - | Roll | HW SemiGlPhoto2 | Heavywght SemiGlos Photo Paper 2 | BK | Temperature 59-86°F Humidity 10-80% | Applicable
Premium Glossy Paper 280 (*1) | Premium Glossy Paper 280 (†) | Roll | Premium Gl 280 | Premium Glossy Paper 280 | BK | Temperature 59-86°F Humidity 30-80% | Applicable
Premium Semi-Glossy Paper 280 (*1) | Premium Semi-Glossy Paper 280 (†) | Roll | Prem.SemiGl 280 | Premium Semi-Glossy Paper 280 | BK | Temperature 59-86°F Humidity 30-80% | Applicable
Poster Semi-Glossy Photo Paper (*1) | - | Roll | Poster Semi-Gl | Poster Semi-Glossy Photo Paper | BK | Temperature 59-86°F Humidity 30-60% | Applicable
Glossy Photographic Paper 190gsm (*1) | Glossy Photographic Paper 190gsm | Roll | GlossyPhoto 190 | Glossy Photographic Paper 190gsm | BK | Temperature 59-86°F Humidity 30-60% | Applicable
Satin Photographic Paper 190gsm (*1) | Satin Photographic Paper 190gsm | Roll | SatinPhoto 190 | Satin Photographic Paper 190gsm | BK | Temperature 59-86°F Humidity 30-60% | Applicable
Glossy Photographic Paper 240gsm | Glossy Photographic Paper 240gsm | Roll | GlossyPhoto 240 | Glossy Photographic Paper 240gsm | BK | Temperature 59-86°F Humidity 30-60% | Applicable
Satin Photographic Paper 240gsm | Satin Photographic Paper 240gsm | Roll | SatinPhoto 240 | Satin Photographic Paper 240gsm | BK | Temperature 59-86°F Humidity 30-60% | Applicable
Premium RC Photo Luster | Premium RC Photo Luster, 10 mil | Roll | RC Photo Luster | Premium RC Photo Luster | BK | Temperature 59-86°F Humidity 30-60% | Applicable
Glossy Photographic Paper 270gsm | Glossy Photographic Paper 270gsm | Roll | GlossyPhoto 270 | Glossy Photographic Paper 270gsm | BK | Temperature 59-86°F Humidity 30-60% | Applicable
Satin Photographic Paper 270gsm | Satin Photographic Paper 270gsm | Roll | SatinPhoto 270 | Satin Photographic Paper 270gsm | BK | Temperature 59-86°F Humidity 30-60% | Applicable
HW Glossy Photo Paper | Heavyweight Glossy Photographic Paper 300gsm | Roll | HW Gloss Photo | HW Glossy Photo Paper | BK | Temperature 59-86°F Humidity 30-60% | Applicable
HW Satin Photo Paper | Heavyweight Satin Photographic Paper 300gsm | Roll | HW Satin Photo | HW Satin Photo Paper | BK | Temperature 59-86°F Humidity 30-60% | Applicable
*1: This paper can be used in the Ambient Light Matching Mode. For details on the Ambient Light Matching Mode, refer to the printer's User Manual.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Glossy Photo Paper | 10 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
14 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
50 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
A2 | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
A1 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
A0 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
B2 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
Semi-Glossy Photo Paper | 10 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
14 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
50 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
A2 | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
A1 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
A0 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
B2 | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Premium Glossy Paper 200 | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Premium Semi-Glossy Paper 200 | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Heavyweight Glossy Photo Paper 2 | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
44 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
50 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Heavywght SemiGlos Photo Paper 2 | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
44 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
50 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Premium Glossy Paper 280 | 10 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
50 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Premium Semi-Glossy Paper 280 | 10 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
50 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Poster Semi-Glossy Photo Paper | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
Glossy Photographic Paper 190gsm | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Satin Photographic Paper 190gsm | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Glossy Photographic Paper 240gsm | 16 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Satin Photographic Paper 240gsm | 16 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Premium RC Photo Luster | 16 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
Glossy Photographic Paper 270gsm | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
Satin Photographic Paper 270gsm | 17 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
HW Glossy Photo Paper | 16 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
HW Satin Photo Paper | 16 in. | Yes | Yes | No | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
24 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
42 in. | Yes | Yes | Yes | Off | Required | 100 mm | 100 mm | 100 mm | 100 mm | No
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper.
Synthetic Paper
Highly economical synthetic paper using polypropylene-based film, a material suited for display posters. Can be displayed outdoors if laminated. Product Specifications
Category | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Synthetic Paper | Roll | Syn. Paper | Synthetic Paper | MBK | Temperature 59-86°F Humidity 30-80% | Applicable
Adhesive Synthetic Paper | Roll | Adh. Syn. Paper | Adhesive Synthetic Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Precautions If print quality is your priority, turn off the auto cutting function and stop the printer after printing. We recommend supporting the document with your hands to prevent it from dropping before you press the Stop button and cut the paper. Adhesive Synthetic Paper If the leading edge of Adhesive Synthetic Paper curls upward, the adhesive may stick to the printhead and damage it. In this case, take measures to straighten the paper, such as by cutting the leading edge.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Synthetic Paper | 24 in. | No | Yes | Yes (*3) | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes (*3) | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes (*3) | Off | Required | 100 mm | 100 mm | - | - | No
50 in. | No | Yes | Yes (*3) | Off | Required | 100 mm | 100 mm | - | - | No
Adhesive Synthetic Paper | 24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
50 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper. *3: Media Take-up unit can be used up to max. 60% humidity.
Film
Print on the glossy, translucent front. With light shined from the back, it s used for indoor illumination signboards and vivid displays. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Backlit Film | - | Roll | Backlit Film | Backlit Film | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Backprint Film | Mirror Backlit Film Reverse Print 125 glossy 3633 | Roll | Backprint Film | Backprint Film | BK | Temperature 59-86°F Humidity 30-80% | Applicable
Durable Backlit Film | Durable Backlit Film | Roll | Durable BL Film | Durable Backlit Film | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Precautions Avoid using Backlit Film where the print surface becomes wet. If the media will be used in a humid environment, perform lamination or other appropriate treatments after printing. When printing on Backlit Film, set Print Quality to Standard or High in the printer driver. Printing may appear uneven, but this effect will be softened by backlighting.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Backlit Film | 24 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
36 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
42 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
Backprint Film | 24 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
36 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
42 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
50 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
Durable Backlit Film | 24 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
36 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
42 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
50 in. | No | Eject cut | Yes | Off | Required | 100 mm | 150 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper.
Fabric
Suitable for banners. Fabric banners can be posted outdoors for a short period of time. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Flame-Resistant Cloth | - | Roll | Flame-Res.Cloth | Flame-Resistant Cloth | MBK | Temperature 59-86°F Humidity 10-60% | Not recommended
Fabric Banner | - | Roll | Fabric Banner | Fabric Banner | MBK | Temperature 59-86°F Humidity 30-60% | Not recommended
Thin Fabric Banner | - | Roll | ThinFab.Banner | Thin Fabric Banner | MBK | Temperature 59-86°F Humidity 10-60% | Not recommended
Durable Banner | Durable Banner | Roll | Durable Banner | Durable Banner | MBK | Temperature 59-86°F Humidity 10-60% | Applicable
Precautions Cut off any frays neatly from the edge with scissors or similar instrument. The fibers of a frayed edge may cause entanglement within the printer, resulting in malfunction.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Flame-Resistant Cloth | 24 in. | Yes (two sides only) | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
36 in. | Yes (two sides only) | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
42 in. | Yes (two sides only) | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
50 in. | No | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
59 in. | No | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
Fabric Banner | 36 in. | Yes (two sides only) | Yes | Yes | Off | Not required | 350 mm | 450 mm | - | - | No
42 in. | No | Yes | Yes | Off | Not required | 350 mm | 450 mm | - | - | No
50 in. | No | Yes | Yes | Off | Not required | 350 mm | 450 mm | - | - | No
59 in. | No | Yes | Yes | Off | Not required | 350 mm | 450 mm | - | - | No
Thin Fabric Banner (*3) | 42 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
50 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Durable Banner | 24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
60 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper. *3: By default, NearEnd RollMrgn on the printer is set to 20mm, but you can also change it to 5mm. If you specify 5mm, for best results, use the printer under the recommended environmental conditions.
Proofing
Proofing paper supports the color reproduction gamut for proof offset printing, providing color comparable to a print finish. It is best suited for color proofing print for printing tasks. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Proofing paper (*1) | - | Roll | Proofing Paper | Proofing paper | BK | Temperature 59-86°F Humidity 30-80% | Not recommended
Commercial Proofing Paper (*1) | Commercial Proofing Paper 200gsm | Roll | Comm Proofing | Commercial Proofing Paper | BK | Temperature 59-86°F Humidity 30-80% | Not recommended
Commercial RC Proofing 210gsm | Commercial RC Proofing 210gsm | Roll | RC Proofing 210 | Commercial RC Proofing 210gsm | BK | Temperature 59-86°F Humidity 30-60% | Not recommended
Commercial RC Proofing 270gsm | Commercial RC Proofing 270gsm | Roll | RC Proofing 270 | Commercial RC Proofing 270gsm | BK | Temperature 59-86°F Humidity 30-60% | Not recommended
Precautions If print quality is your priority, turn off the auto cutting function and stop the printer after printing. We recommend supporting the document with your hands to prevent it from dropping before you press the Stop button and cut the paper. Leaving paper loaded in the Media Take-up Unit for extended periods may adversely affect the print quality. We recommend removing paper from the printer if you do not intend to print for a long period of time. If you wish to print with paper left loaded for a long time, press the Online button to bring the printer offline. Then press the ▼ key to feed the paper about 50 mm (2.0 in) and start printing.
*1: This paper can be used in the Ambient Light Matching Mode. For details on the Ambient Light Matching Mode, refer to the printer's User Manual.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Proofing Paper | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
24 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
42 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Commercial Proofing Paper | 24 in. | No | Yes | Yes | Off | Required | 100 mm | 320 mm | - | - | Yes
36 in. | No | Yes | Yes | Off | Required | 100 mm | 320 mm | - | - | Yes
Commercial RC Proofing 210gsm | 24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | Yes
Commercial RC Proofing 270gsm | 24 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | Yes | Off | Required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper.
Art Paper
Art paper that expands the potentials of large-format ink jet printing. Provides a placid and high-definition image quality in various applications from portrait, landscape and watercolor to digital art works. Canvas is a polyester woven fabric-based cloth with a unique feel. Available in matte and semi-glossy types, it is best suited for reproduction of oil and other paintings and prints of painting-like digital art works. Japanese paper washi offers compatibility between ink jet print suitability and traditional washi look and feel. This paper is a good choice to convey a feeling of warmth and a somewhat subdued effect in artwork or point-of-purchase displays depicting watercolor pictures, ink drawings, or art with an Asian touch. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
Fine Art Photo Paper | Fine Art Photo Paper "Photo Rag™" 188 (†) | Roll | FineArt Photo | Fine Art Photo | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Photo Rag 188g | Roll | FineArt Photo | Fine Art Photo | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Heavyweight Photo Paper | Photo Rag 308g | Roll | FneArt HW Photo | Fine Art Heavyweight Photo | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Textured Paper | German Etching 310g | Roll | FineArt Txtr | Fine Art Textured | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Watercolor | - | Roll | FineArt Wtrclr | Fine Art Watercolor | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Block Print | - | Roll | FineArtBlockP | Fine Art Block Print | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Enhanced Velvet 255g | Fine Art Enhanced Velvet 255gsm | Roll | FA Enha. V. 255 | Fine Art Enhanced Velvet 255g | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Natural 230g | Fine Art Natural 230g | Roll | FA Natural 230 | Fine Art Natural 230g | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Bright White 230g | Fine Art Bright White 230g | Roll | BrightWhite 230 | Fine Art Bright White 230g | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Fine Art Bright White 330g | Fine Art Bright White 330g | Roll | BrightWhite 330 | Fine Art Bright White 330g | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Graphic Canvas | Graphic Matte Canvas | Roll | Graphic Canvas | Graphic Canvas | MBK | Temperature 59-86°F Humidity 10-60% | Not recommended
Canvas Matte | Canvas Artist 340g | Roll | Canvas Matte | Canvas Matte | MBK | Temperature 59-86°F Humidity 10-60% | Not recommended
Japanese Paper Washi | - | Roll | JPN Paper Washi | Japanese Paper Washi | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
Precautions If print quality is your priority, turn off the auto cutting function and stop the printer after printing. We recommend supporting the document with your hands to prevent it from dropping before you press the Stop button and cut the paper. Fine Art Block Print Fine Art Block Print art paper is not guaranteed to be compatible with borderless printing without borders on all four sides. It is compatible only with borderless printing without borders on two sides. However, before this kind of borderless printing, set CutDustReduct. to On in the MAIN MENU. For details, refer to the printer's User Manual. Canvas Matte Cut off any frays neatly from the edge with scissors or similar instrument. The fibers of a frayed edge may cause entanglement within the printer, resulting in malfunction.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
Fine Art Photo Paper | 24 in. (*3) | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. (*4) | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
44 in. (*4) | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Fine Art Heavyweight Photo Paper | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | Yes
44 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | Yes
Fine Art Textured Paper | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
44 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Fine Art Watercolor | 17 in. | No | Yes | Yes | 60 sec. | Not required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | 60 sec. | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | 60 sec. | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
Fine Art Block Print | 17 in. | No | Yes | Yes | 60 sec. | Not required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | 60 sec. | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | 60 sec. | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
Fine Art Enhanced Velvet 255g | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
44 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
50 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Fine Art Natural 230g | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
60 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Fine Art Bright White 230g | 17 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | Yes | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
60 in. | No | Yes | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Fine Art Bright White 330g | 17 in. | No | No | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | Yes | No | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
36 in. | Yes | No | Yes | Off | Not required | 100 mm | 100 mm | 100 mm | 100 mm | No
60 in. | No | No | Yes | Off | Not required | 100 mm | 100 mm | - | - | No
Graphic Canvas (*5) | 17 in. | No | Eject cut | Yes | Off | Required | 100 mm | 200 mm | - | - | No
24 in. | Yes (two sides only) | Eject cut | Yes | Off | Required | 100 mm | 200 mm | - | - | No
36 in. | Yes (two sides only) | Eject cut | Yes | Off | Required | 100 mm | 200 mm | - | - | No
42 in. | Yes (two sides only) | Eject cut | Yes | Off | Required | 100 mm | 200 mm | - | - | No
50 in. | No | Eject cut | Yes | Off | Required | 100 mm | 200 mm | - | - | No
60 in. | No | Eject cut | Yes | Off | Required | 100 mm | 200 mm | - | - | No
Canvas Matte | 36 in. | Yes (two sides only) | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
44 in. | No | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
50 in. | No | Yes | Yes | Off | Not required | 100 mm | 200 mm | - | - | No
Japanese Paper Washi | 17 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper. *3: For Fine Art Photo Paper "Photo Rag™" 188 only. *4: For Photo Rag 188g only. *5: By default, NearEnd RollMrgn on the printer is set to 20mm, but you can also change it to 5mm. If you specify 5mm, for best results, use the printer under the recommended environmental conditions.
CAD Paper
This paper is a good choice for CAD graphic (line drawing) prints. CAD Tracing Paper is thin, translucent paper that can be used in color printing. CAD Translucent Matte Film offers high dimensional stability, making it suited for high-precision prints such as master drawings. Product Specifications
Category | Product Name | Type | Control Panel | Printer Driver | Black Ink | Recommended Environment | Laminate
CAD Tracing Paper | - | Roll | CAD Trace Paper | CAD Tracing Paper | MBK | Temperature 59-86°F Humidity 30-80% | Not recommended
CAD Translucent Matte Film | - | Roll | CAD Matte Film | CAD Translucent Matte Film | MBK | Temperature 59-86°F Humidity 10-80% | Not recommended
CAD Clear Film | - | Roll | CAD Clear Film | CAD Clear Film | BK | Temperature 59-86°F Humidity 30-60% | Not recommended
Economy Bond Paper | Economy Bond Paper | Roll | Economy Bond | Economy Bond Paper | MBK | Temperature 59-86°F Humidity 30-60% | Applicable
Universal Bond Paper | Universal Bond Paper | Roll | Universal Bond | Universal Bond Paper | MBK | Temperature 59-86°F Humidity 10-80% | Applicable
Precautions CAD Tracing Paper Remove each sheet upon ejection into the output tray. Do not touch the print surface or stack sheets before ink dries. Avoid using CAD Translucent Matte Film and CAD Tracing Paper where they become wet. CAD Clear Film If you are using automatic detection of the remaining roll paper with CAD Clear Film, before printing, manually cut the portion of the film that includes the media name or other text.
Roll Specifications
Category | Size | Borderless Printing | Auto Cutting | Media Take-up Unit | Ink Drying Time | Edge Precut Paper Removal | Edge Precut Length | Color Calibration (*2)
When loading paper (*1) | Borderless printing
Normal humidity | Low/High humidity | Normal humidity | Low/High humidity
CAD Tracing Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A2 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A1 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
A0 | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
CAD Translucent Matte Film | 36 in. | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | No
A1 | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | No
A0 | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | No
CAD Clear Film | 36 in. | No | Eject cut | No | Off | Required | 100 mm | 100 mm | - | - | No
Economy Bond Paper | 24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
Universal Bond Paper | 17 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
24 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
36 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
42 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
60 in. | No | Yes | No | Off | Not required | 100 mm | 100 mm | - | - | No
*1: Paper is cut when you have selected On for Trim Edge First in the printer menu. If you have selected Automatic for Trim Edge First, the printer will determine the state of the leading edge and cut the paper automatically as needed. Automatic is the default setting for most types of paper. *2: Paper labeled with "No" cannot be used to perform color calibration (that is, to print the patterns for adjustment). However, the adjustment value from calibration using paper labeled with "Yes" will also be used as the basis for adjustment for these types of paper.
Type: | Shows the paper type. The properties are given in a separate table according to the type.
Control Panel: | Shows the paper types selected in Roll Media Type and Cut Sheet Type, the options set on the control panel.
Printer Driver: | Shows the paper types selected in Media Type of the printer driver.
Black Ink: | Shows the black ink types used.
Recommended Environment: | Shows the temperature and humidity ranges for using paper.
Laminate: | Shows whether ordinary cold lamination is applicable.
Borderless Printing: | Shows whether borderless printing is possible.
Auto Cutting: | Shows the method of paper cutting.
Media Take-up Unit: | Indicates that the media take-up unit cannot be used.
Ink Drying Time: | Shows the ink drying time when using the cutter. Set the printer's ink drying time according to this table.
Edge Precut Paper Removal: | Required is indicated for paper for which you must remove scraps produced when the leading edge is cut. Remove these scraps from the platen or output stacker before printing.
Edge Precut Length: | Indicates the edge precut length for roll paper.
Color Calibration: | Indicates whether the paper can be used for color calibration.
Precautions: | Shows the precautions and limitations for each paper type.
The information given here is current as of end of August, 2008 and subject to change at any time.
To purchase paper, contact your printer distributor.
Copyright Canon Inc. 2008