
This README file contains the latest information about your EPSON product.

--------------------------------------------------
EPSON HDI Driver Plotter Configuration README File
--------------------------------------------------

Copyright (C) SEIKO EPSON CORPORATION, 2012

____________________________________________________________________________________________

After installing the HDI driver, follow the steps below to create a plotter configuration 
file. For detailed information, refer to AutoCAD Help in the Help menu.

1.  Start AutoCAD or AutoCAD LT.
2.  Select Plotter Manager from the File menu. The Plotters folder opens.
3.  Double-click the Add-A-Plotter Wizard icon. The Add Plotter dialog box appears. 
    After reading the Introduction Page, click the Next button.
4.  Select My Computer, then click the Next button.
5.  Select EPSON in the Manufacturers list box, then select your printer in the Models 
    list box (See Note below). Click the Next button.
6.  Follow the on-screen instructions to complete the steps. When the Add Plotter - Finish 
    screen appears, click the Finish button. The plotter configuration file is added to 
    the Plotters folder.
7.  Click the close button (the "x" button) in the upper right corner of the Plotters 
    folder window to close the window.

Note: In step 5, if EPSON is not displayed in the Manufacturers list box, or if the HDI
      driver was installed in a place other than \ProgramFiles\AutoCAD\, create the 
      plotter configuration file  by following the steps below.

1.  Close Add-A-Plotter Wizard.
2.  Start Explorer.
3.  Open the folder in which the HDI driver was installed, then open the DRV folder. Copy
    all of the files in this folder and paste them into the DRV folder in the AutoCAD or
    AutoCAD LT folder.
4.  Using the same method, open the HELP folder for the HDI driver. Copy all of the files 
    in this folder and paste them into the HELP folder in the AutoCAD or AutoCAD LT folder.
5.  Start AutoCAD or AutoCAD LT.
6.  Select Plotter Manager from the File menu. The Plotters folder opens.
7.  Double-click the Add-A-Plotter Wizard icon. The Add Plotter dialog box appears. 
    After reading the Introduction Page, click the Next button.
8.  Select My Computer, then click the Next button.
9.  Select EPSON in the Manufacturers list box, then select your printer in the Models 
    list box. Click the Next button.
10. Follow the on-screen instructions to complete the steps. When the Add Plotter - Finish
    screen appears, click the Finish button. The plotter configuration file is added to 
    the Plotters folder.
11. Click the close button (the "x" button) in the upper right corner of the Plotters 
    folder window to close the window.
