## Using the Setup menu

Notes:

- Printer settings selected from a program or printer driver override default settings.
- Options and settings may vary depending on the printer.

Menu item | Description | Settings
--- | --- | ---
Printer Language | Defines the default printer language used to communicate data from the computer to the printer Note: Setting one printer language as the default does not prevent a program from sending print jobs that use the other language. | PCL Emulation PS Emulation PPDS Emulation
Jam Recovery | Specifies whether or not the printer always reprints a jammed page (On), never reprints a jammed page (Off), or reprints a jammed page unless the memory required to hold the page is needed for other printer tasks (Auto) Note: Auto is the default setting. | On Off Auto
Display Language | Specifies the language of the text on the printer control panel display Note: All languages may not be available. The default language for your country or region is set at the manufacturer. | English Francais Deutsch Italiano Español

Dansk

Norsk

Nederlands

Svenska

Portugues

Suomi

Japanese

Russian

Polski

Hungarian

Turkish

Czech

Korean

Simplified Chinese

Traditional Chinese

Print Area | Modifies the logical and physical printable area Notes:

- Normal is the default setting. When attempting to print data in the non-printable area defined by the Normal setting, the printer clips the image at the boundary.
- The Whole Page setting only affects pages printed using the HBP interpreter. This setting has no effect on pages printed using the PCL interpreter or PostScript interpreter.

Normal

Whole Page

Alarm Control | Specifies whether and how often the printer sounds an alarm when the printer requires operator intervention Notes:

- Single is the default setting. The printer sounds three quick beeps.
- When Off is set, the printer does not sound an alarm.
- When Continuous is set, the printer repeats three beeps every 10 seconds.

Off

Single

Continuous

Toner Alarm | Specifies whether the printer should stop printing and activate either a single or continuous alarm when a toner low condition occurs Notes:

- Off is the default setting. When Off is set, the printer does not sound an alarm.
- When Single is set, the printer sounds three quick beeps.
- When Continuous is set, the printer repeats three beeps every 10 seconds.

Off

Single

Continuous

Download Target | Specifies the storage location for downloaded resources Notes:

- RAM is the default setting. All downloaded resources are automatically stored in printer memory.
- Storing downloaded resources in flash memory is permanent storage rather than the temporary storage that RAM provides

RAM

Flash

Power Saver | Sets the amount of time (in minutes) the printer waits after a job is finished before it goes into a reduced power state Note: Selecting 1–240 specifies the amount of time after a print job before the printer goes into Power Saver mode. The range of values varies by printer. | 1–240
Print Timeout | Specifies the amount of time (in seconds) the printer waits before printing the last page of a print job that does not end with a command to print the page Notes:

- Disabled is the default setting.
- 90 is the default range setting.

Disabled

1–255

Auto Continue | Defines the amount of time (in seconds) the printer waits after displaying an operator intervention error message before it resumes printing Notes:

- Disabled is the default setting. The printer does not resume printing until the error message is cleared.
- When you specify a range setting, the printer waits the specified amount of time and then automatically resumes printing.
- Five is the default range setting.

Disabled

5–255

Wait Timeout | Specifies the amount of time (in seconds) the printer waits to receive additional bytes of data from the computer Notes:

- Disabled is the default setting.
- 40 is the default range setting.
- When this timeout expires, the print job is canceled. Wait Timeout is only available when you use PostScript emulation. This menu item has no effect on HBP, PPDS, or PCL emulation print jobs.

Disabled

15–65535

Resolution Reduction | Specifies whether the printer automatically reduces 600 dpi pages to 300 dpi pages to prevent memory full situations | Off On
Resource Save | Specifies whether all permanent downloaded resources, such as fonts and macros stored in RAM, are saved if the printer receives a job that requires more memory than is available Note: Off is the default setting. The printer retains downloaded resources only until memory is needed. It then deletes those resources associated with the inactive printer language. | Off On
Reset Control | Specifies whether the Reset function is available when you press and hold the printer Cancel button Notes:

- On is the default setting.
- Print jobs stored in the printer memory may be fully or partially lost when the printer is reset.

Off

On

Print Buffer Control | Specifies whether the control panel Print Buffer function is available on the printer Note: On is the default setting. | Off On
Page Protect | Prevents the printer from picking paper for a page until the entire page is processed and ready to be printed Notes:

- Off is the default setting. The printer prints a partial page when there is not enough memory to print the entire page.
- On sets the printer to process the whole page so that the entire page prints.

Off

On

Eco-Mode | Conserves the amount of energy and/or supplies used Notes:

- Off is the default setting. The printer is at its best performance level.
- The Energy setting conserves energy usage, calling upon the absolute minimum required.
- The Paper setting minimizes paper waste.
- The Energy/Paper setting minimizes waste of paper, toner, and energy, using the minimum requirements.

Off

Energy

Paper

Energy/Paper

Quiet Mode | The printer operates in a reduced noise mode. Note: Off is the default setting. | Off On