
*** The Color Ink-jet printer MJC-640A by SAMSUNG ***
           (DOS version README)

-------------------
DOS-READ.ME CONTENTS
-------------------

- Overview

- Compatibility and System Requirements

- Installing & Running MJRCP (The Color Ink-jet printer
  MJC-640A DOS Remote Control Panel)

- User Tips and Recommendations

- Loading Special Media

- Problem Determination

This text file, DOS-READ.ME, provides additional
information to help you.

Use the SAMSUNG Color Ink-jet printer MJC-640A. If you
need further technical assistance, contact your point of
purchase or your SAMSUNG country representative.

--------
OVERVIEW
--------

Q:      What is MJRCP(DOS Remote Control Panel)?

A:      MJRCP refers to the "MJRCP.EXE" program that
        allows you to control your Color Ink-jet printer
	MJC-640A from DOS much as you would control it
        through the Printer Setup screen in Windows.

        If you intend to use the Color Ink-jet printer
        MJC-640A from within a DOS application you will
        need to make printer setting adjustments using
        this utility.

        Some things you can do from within the MJRCP
        program are:

        -  Verify your printer to computer connection

        -  Set paper type and size

        -  Set print margins and orientation

        -  Clean and align ink cartridges

-------------------------------------
COMPATIBILITY AND SYSTEM REQUIREMENTS
-------------------------------------

The MJRCP Utility was designed and tested for the
following PC operating systems and environments:

- PC-DOS or MS-DOS versions 5.0 or higher

- Microsoft Windows versions 3.1 or Win 95

If you are running Microsoft Windows, you must close
Windows before installing MJRCP - the Color Ink-jet
printer MJC-640A DOS Remote Control Panel.

------------------------------------
RUNNING THE DOS REMOTE CONTROL PANEL 
------------------------------------

To install MJRCP-the Color Ink-jet printer DOS utility:

  - If you are running Microsoft Windows, either close
    Windows or start a full screen DOS session.  Note:
    INSTALL may not function correctly in a windowed DOS
    session.

  - Insert the diskette labeled "Program Disk 1" into
    drive A:.

  - At the DOS command prompt, type A:INSTALL and press
    Enter.

  - Follow the directions displayed on the screen.

To run MJRCP-the Color Ink-jet printer DOS utility:

  - If you are running Microsoft Windows, either close
    Windows or start a full screen DOS session.  Note:
    MJRCP may not function correctly in a windowed DOS
    session.

  - At the DOS command prompt, type C:\MYJET\MJRCP and
    press enter.

  - Follow the directions displayed on the screen.

-----------------------------
USER TIPS AND RECOMMENDATIONS
-----------------------------

  GENERAL

- You should make backup copies of the diskettes in case
  your original diskettes are damaged during use.  You
  can use the DOS DISKCOPY command to copy the diskettes.
  Keep these diskettes with your printer and printer
  documentation.

- The setting in the MJRCP may be overridden by your
  DOS application. Whenever possible you should use the
  DOS application to change settings for a document.
  MJRCP settings should be used to change settings when
  an application does not have that function.

- The Current Settings reported by MJRCP are the
  default settings for the printer. These settings may
  not reflect the current state of the printer. The cur-
  rent state of the printer is set to the default set-
  tings whenever the printer is turned on, when a reset
  command is sent to the printer or when you use MJRCP
  to interact with the printer (except to read the set-
  tings).

- The minimum top margin in landscape orientation is 0.25
  inches.

---------------------
LOADING SPECIAL MEDIA
---------------------

Follow the steps below to load thick paper, envelopes,
or other special media in the sheet feeder.

1. Remove any paper in the sheet feeder.
2. Open the envelope guide to an upright position.
3. Place the special media against the envelope guide 
   in the sheet feeder.
4. Move the paper guide to the right until it rests
   against the special media.
5. Guide the special media down into the sheet feeder
   until it begins to feed.

NOTE: Return the envelope guide to its original position
      when not printing special media.

---------------------
PROBLEM DETERMINATION
---------------------

- NOT ENOUGH MEMORY TO RUN SETUP

  If the message "You do not have enough memory to run
  the utility" appears when you run Setup, increase the
  amount of free memory in your DOS session.

(See the MS DOS reference guide for more information on
how to free up and configure memory for DOS applications)

- MOUSE NOT WORKING

  The Setup and Toolkit for DOS support mouse input.  To
  enable mouse support, load the mouse driver provided
  with your mouse before using the Printer Setup or
  Toolkit.

- CRITICAL DISK ERROR USUALLY MEANS WRITE PROTECT ERROR

  Critical Disk Errors when using the DOS Utilities are
  typically due to the diskette or Network Drive being
  Write Protected.

==========================================================
* MS DOS, Windows and Win 95 are trademarks or registered
  trademarks of Microsoft Corp.
* PCL, HP 500 and HP 500C are trademarks or registered
  trademarks of Hewlett-Packard Company
==========================================================

------------------
END OF DOS-READ.ME
------------------
