## Using the PCL Emulation menu

Notes:

- Printer settings selected from a program or printer driver override default settings.
- Options and settings may vary depending on the printer.

Menu item | Description | Settings
--- | --- | ---
A4 Width | Specifies the width of the logical page for A4-size paper Note: 198 mm is the default setting. | 198 mm 203 mm
Orientation | Specifies how text and graphics are oriented on the page Note: Portrait is the default setting. | Portrait Landscape
Auto CR after LF | Specifies whether the printer automatically performs a carriage return after a line feed control command Note: Off is the default setting. | Off On
Auto LF after CR | Specifies whether the printer automatically performs a line feed after a carriage return control command Note: Off is the default setting. | Off On
Lines Per Page | Specifies the number of lines that print on each page Notes:

- 60 is the US default setting. 64 is the non-US default setting.
- The printer sets the amount of space between each line based on the Lines per Page, Paper Size, and Orientation menu items. Select the correct Paper Size and Orientation before changing Lines per Page.

1–255

Tray Renumber > Assign Tray <x> | Configures the printer to work with printer drivers or programs that use different source assignments for the paper trays (input sources) Note: Off is the default setting. | Off 0–199
Tray Renumber > Assign Manual Paper | Configures the printer to work with printer drivers or programs that use different source assignments for the manual feeder Note: Off is the default setting. | Off 0–199
Tray Renumber > Assign Manual Envelope | Configures the printer to work with printer drivers or programs that use different source assignments for the manual envelope feeder Note: Off is the default setting. | Off 0–199